

RFID Tag

• Contains a microchip & antenna which is tagged to the Easylube grease lubricator  
• Transmits bearing lubrication status to the handheld PDA  
• It enables real time tracking of lubrication to achieve maintenance excellence  
• Assuring the entire plant lubrication program is well managed





Warranty – Quality Assured – 2 Year Warranty on Easylube products. No other automatic lubricator on the market even comes close.



Electro-Mechanical Unit – driven by electricity (not by gas, chemicals or spring driven)



Filled with Grease of Choice – very cost effective



Temperature Range – from -12C to 90C – PROVEN that it is not affected by temperature fluctuations



Connection Thread – made of durable BPA flex 1.2″ (M) strong thread that will not easily break



Battery Type – is a 6V Lithium battery pack (not used in any household items or toys)



Visible Indicator – a warning light flashes when grease supply is exhausted or if a feed blockage occurs



Remote Mounting – Remote mounting (up to 4.572m away) and quick connections allow lubricators to service difficult to reach grease points, ensuring maintenance is both simple and safe



Software is equipped with a built-in RFID (Radio Frequency Identification) reader and MQL software



Operating Pressure

• Lubricant quality and quantity is guaranteed with Easylube – the most accurate lubricator on the market!  
• 75-150 psi (5-10 bar) – Tested – output pressure self adjusts for the pipeline  
• Impulse lubrication reduces the risk of over-lubrication  
• Each lube point’s grease feed rate and condition is tracked by the Guardwatch/Skymonitor APP on your mobile device



Easylube Guardwatch Service & Maintenance Software and Reports

• General Records to check bearing abnormality and missed inspections  
• Pre-warning monitor to check grease balance and date of replacement  
• Pre-warning monitor displays a warning light (red) 15 days before due date of replacement



Refill Kit

• Drive unit can be used repeatedly with the new lithium battery pack  
• Special designed refill kit  
• Economical and reliable  
• Grease capacity of 150ml and 250ml  
• Eliminate manual recording mistakes – giving you up to date bearing lubrication information  
• Specific grease feed tracking rate in each single lube-point on site



Tax Benefit – The Easylube Lubricator is classified as a machine or a tool (not a disposable unit) – so it can be claimed as a taxable item.